A vehicle is considered to be technically incapable for traffic on road communications, if
a) it is fitted with tyres of different dimensions and constructions,
b) the lowest point of active lighting surface of brake-lights is higher than 350 mm above the level of the road,
c) distance meter is out of order.
