If during towing of a motor vehicle a bar is used, it must be evidently marked
a) by diagonal yellow and black stripes with width at least 10 cm,
b) by diagonal red and white stripes with width 7.5 cm,
c) by slanted red stripes.
