A vehicle is considered to be technically incapable for road communication traffic, if
a) some of light signalling devices, important for safety of traffic on road communications
is missing or is placed not correctly, does not glow or does not fulfil prescribed conditions, c so that there is threat of imminent danger,
b) the highest point of active luminous area of low-beam reflectors is lower than 1200 mm above level of the carriageway,
c) the vehicle is not equipped by an air-conditioning system.
