A vehicle is considered to be technically incapable for traffic on road communications, if
a) mud-flaps are damaged,
b) distance-meter is out of order,
c) non-identical tyres on the same axle are used.
