When motor vehicle is towed by using a rope, it must be visibly marked
a) with a red flag or label with dimensions at least 20 * 20 cm,
b) with a yellow flag and label with dimensions at least 25 x 25 cm,
c) at reduced visibility by a red non-dazzling light.
