A driver must not enter the railway crossing, if
a) the oncoming driver gives an audible warning sign,
b) warning is given by interrupted sound of a horn or a bell of a railway crossing security equipment,
c) a person taken on for ensuring safe operation of the railway crossing gives instruction by horizontal waving of his hand with a red or yellow flag.
