A vehicle is considered to be technically incapable for road communication, if
a) additionally mounted light equipment obstructs the view from the place of passenger,
b) the lowest point of the active lighting area of brake-lights is higher than 350 mm over road level,
c) some of the light equipment necessary for traffic safety on road communications
are missing or are situated incorrectly, do not work or do not meet the specified conditions, thus direct danger threatens.
