If it is necessary to give warning of impending danger to other participants of the road traffic, especially in situations when Is required sudden reduction of speed or to bring vehicle to a stop,
a) driver gives a warning sign by activation of a warning function of turn-signal lights,
b) driver will use acoustic warning sign,
c) driver gives a warning sign by interrupted activation of the front fog lights.
