If fuel, oil, or other fillings necessary for operation are evidently leaking from the vehicle
a) driving by this vehicle is possible only at speed not exceeding 60 km.h-1,
b) such vehicle is considered to be technically incapable for traffic on road communications,
c) such vehicle can be used only on tertiary communications.
