If gates are being lowered, or are lowered or if are lifting, a driver
a) may enter the railway crossing, if dimensions of his vehicle enable it,
b) may enter the railway crossing, if no train can be seen,
c) must not enter the railway crossing.
