Compulsory equipment of a motor vehicle of M, N, T, C and Ps, category are
a) at least a ten-litre reserve of fuel and at least a two-litre reserve of cooling liquid in separate containers; not applicable for one-track motor vehicles,
b) nuts and bolts for dimension of wheel designated by manufacturer,
c) homologized portable warning triangle.
