A vehicle is considered to be technically incapable for traffic on road communications, if
a) some of the light equipment necessary for safety of traffic on road communications
are missing or are incorrectly located, does not glow or fail to meet the specified conditions, thus direct danger threatens,
b) catalyser of exhaust gases is beyond calibration expiry,
c) the highest point of active lighting area of brake lights is lower than 1500 mm above the road level.
