Compulsory equipment of a motor vehicle of M and N category is
a) at least ten-litre reserve of fuel in separate containers,
b) towing bar with length at least 3 m, designated for towing vehicles,
c) hand lift-jack with weight equalling at least to loading of the most loaded axle of the vehicle or equalling to the weight of the lifted part of the vehicle with max. permissible overall weight of vehicle at lifting of this part by a method specified by manufacturer for using the lift-jack.
