A vehicle operator must not operate a vehicle in traffic on land communication that
a) is additionally equipped by uncertified system, component or individual technical unit,
b) does not have at least tyres of front axle fitted with effective covers (fenders, arches),
c) has additionally fitted approved light equipment, obstructing the view from the seat of the passenger.
