An operator must not in traffic on road communications operate a vehicle
a) that does not reach the min. speed of 100 km.h-1,
b) that damages road communications beyond acceptable level,
c) of which lights in the baggage area are not functional.
