A vehicie is considered to be technically incapable for traffic on road Communications, if
a) on the same axle different tyres are used,
b) the lowest point of active lighting area of parking lights is higher than 350 mm over carriageway level,
c) it is not possible to switch high-beam headlights to parking lights.
