A vehicle is considered to be technically incapable for road communication, if
a) the tone of the audible warning sign was changed,
b) the view from the seat of the driver is limited or disabled,
c) mud flaps are damaged.
