The depth of main grooves in the central part of the tyre tread pattern surface, that covers approx, three fourth of the width of the tyre tread pattern surface, must not be less than
a) 1.5 mm in case of passenger cars,
b) 1.6 mm in case of passenger cars,
c) 1.7 mm in case of passenger cars.
