If fuel, oil, or other operating fluids are evidently leaking from the vehicle,
a) driving by such vehicle is allowed only at speed not exceeding 60 km.h-1,
b) such vehicle is considered to be technically incapable for traffic on the road communications,
c) such vehicle can be used only on tertiary roads.
