A vehicle is considered to be technically incapable for traffic on road communications, if
a) additionally fitted light equipment invade the view from the place of a passenger,
b) chassis, frame or bodywork of the vehicle is damaged or deformed,
c) the vehicle is not fitted with equipment for connecting vehicles.
