An operator must not in a traffic on road communications operate a vehicle,
a) of which overall permissible width of the vehicle exceeds 2200 mm,
b) that was not put under emission inspection within one month after the first record to registry
c) that during check of the vehicle originality, if it is subject to such check, was evaluated as being unable for traffic on the road communications.
