The depth of main tyre grooves in the central part of tread pattern surface, that covers approx. three fourth of the width of tyre tread pattern surface, must not be less than
a) 1.5 mm in case of L1e category vehicles,
b) 1.6 mm in case of vehicles of each category,
c) 1.0 mm in case of L1e category vehicles.
