A vehicle is considered to be technically incapable for traffic on road communications, if
a) there is a change in tone of the audible warning equipment,
b) view from the seat of a driver is limited or made impossible,
c) there is no blanking tape on the front window that enables at least 50% permeability of light.
