A vehicle is considered to be technically incapable for traffic on road communications, if
a) on the rear window approved foil is used,
b) lubricant used in a vehicle is not approved by the manufacturer,
c) fuel, oil, lubricant or other fillings operating fluids are evidently leaking from the vehicle.
