A vehicle is considered to be technically inappropriate for road traffic, if
a) catalyser of exhaust gases is beyond calibration expiry,
b) there is no blanking sheet on the front window that enables at least 50 % permeability of light,
c) some part of the exhaust emission system is leaking, thus exhaust gases enter into the area for passengers, driver or load or they are the source of excessive loud.
