If a load on vehicle extends at the front or at the back by more than
a) by 1 m, the extending end of the load must be labelled with a yellow flag with dimensions at least 20 x 20 cm; at reduced visibility at the front and at the back with a yellow reflecting glass,
b) by 40 cm, the extending end of the load must be labelled with a reflecting sign
with red and white stripes of width 70-100 mm and directing from the longitudinal centre plane of a vehicle at 45* angle downwards,
c) by 50 cm, it must be always labelled with a red reflecting glass.
