Tram rail area increased over the road level or decreased under road level, or that is separated from the road otherwise, mainly with a kerb, can be crossed
a) only laterally, and at a place that is adjusted for it,
b) at whatever place, and always laterally,
c) at whatever place, if there is no tram nearby.
