A vehicle is considered to be technically incapable for traffic on road communications, if
a) there is a change in tone of the audible warning equipment,
b) the lowest point of the active lighting area of low-beam headlights is lower than 1200 mm above the road level,
c) some of the lighting equipment necessary for the safety of traffic on road communications is missing or is situated incorrectly, does not work or does not meet the designated conditions, thus immediate danger threatens.
