At breakdown of lighting or other breakdown disabling the use of lighting, at reduced visibility on the towed vehicle must be turned on
a) lights on the side to the centre of the road in the front with white non-dazzling light and in the back with at least one red light,
b) two red lights in the front and in the back,
c) lights inside the vehicle.
