If a load on vehicle extends to a side, the extending end of the load must be labelled
a) by a reflection marking with 70 to 100 mm wide red and white stripes and heading from longitudal centre plane of a vehicle at 45° angle downwards,
b) by a red flag with dimensions at least 30 x 30 cm.
c) always by yellow and black stripes.
