Before turning to the left a driver is obliged to join
a) as much left as possible from that part of the pavement that is designated for his driving direction taking into consideration the dimensions of the vehicle or load and width
of pavement,
b) as much right as possible in that part of pavement that is designated for his driving direction,
c) on the right shoulder.
