A vehicle Is considered to be technically incapable for traffic on road communications, if
a) some of the light equipment necessary for safety of traffic on road communication is missing or it is incorrectly situated, does not work or does not meet the prescribed conditions,
thus immediate danger threatens,
b) the highest point of the active lighting area of brake lights is lower than 1500 mm above the level of the pavement,
c) it is not fitted with equipment for connecting vehicles.
