If during driving a vehicle in a tunnel breakdown of the vehicle occurs, for which this vehicle becomes broken down, or a traffic accident occurs including fire, the driver after stopping the vehicle is obliged immediately to
a) turn off the low-beam headlights,
b) report stopping of the vehicle to the relevant district office,
c) switch off engine.
