The depth of tyre grooves in the central part of tread pattern surface, that covers approx, three fourth of the width of tyre tread pattern surface, must not be less than
a) 1.5 mm in case of passenger cars,
b) 1.6 mm in case of passenger cars,
c) 1.7 mm in case of passenger cars.
