If for towing of a motor vehicle a bar is used, it must be evidently marked
a) by diagonal red and white stripes with width 7,5 cm,
b) by diagonal yellow and black stripes with width at least 10 cm,
c) by slanted red stripes.
