A vehicle is considered to be technically incapable for road communication traffic, if
a) lubricant used in a vehicle is not approved by manufacturer,
b) illumination of the luggage boot can not be activated,
c) the fuel, oil, lubricant or other service liquids apparently leak out of a vehicle.
