This additional panel indicates
a) opening of two consecutive country or forest roads to the road,
b) segment for application of a sign, under which the panel is located,
c) the real shape of two consecutive intersections and the main and the side road.

