A vehicle is considered to be technically incapable for traffic on road communications, if
a) the tyre on its external perimeter has cracks or damages, that expose the textile-cord carcass or invade it,
b) the vehicle is not fitted with at least one searchlight with white-colour light,
c) it is not possible to switch the high-beam headlights to the position lights.
