A vehicle is considered to be technically incapable for traffic on road communications, if
a) distance meter is not functional,
b) condition of the control pedal and its peg or track do not allow safe control of a service brake,
c) at least wheels of the front axle are not fitted with effective covers (mudguards, wheel arches).
