Compulsory equipment of a motor vehicle of M and N category is
a) tow bar with min. length of 6 m designated for towing vehicles,
b) tow rope; it is applied also for one-track vehicles,
c) hand lift-jack with capacity equalling at least to loading of the most loaded axle of the vehicle or equalling to the weight of the lifted part of the vehicle from the max. admissible weight weight
of the vehicle while lifting this part by the designated method specified by the manufacturer
manufacturer
for using lift-jack.
