The vehicle operator must not for traffic on the ground communications use vehicle that
a) is not able to achieve on the flatland a speed of at least 50 km/h,
b) causes damage to the road communications above acceptable level,
c) did not undergo an inspection of its technical condition within period of one month after its first registration.
