Compulsory equipment of a motor vehicle of M, N, T, C and Ps, category are
a) at least two wheel chocks for each axle of the motor vehicle,
b) homologized portable warning triangles,
c) two reserve closed nuts of the wheel bodies.
