If a load extends a vehicle at the front or at the back by more than
a) by 1 m, the extended load end must be marked by a yellow flag with dimensions at least
20 x 20 cm; at reduced visibility both at the front and at the back by a yellow reflecting glass,
b) by 40 cm, the extended load end must be marked by a reflex marking with red and white strips, wide 70 up to 100 mm and directing from vehicle longitudinal central plane under angle of 45* downwards,
c) by 0.5 m; it must always be marked by a red reflecting glass.
